{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["第一标段"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"第一标段","index":0,"n_rows":5,"n_cols":10,"rows_kept":5,"merged":[[0,0,0,9],[4,0,4,1]],"flags":["formulas_cached_only"]}
["安康学院DSP/SOPC实验室仪器设备采购清单"]
[]
["序号","设备名称","品牌","型号","规格","单位","数量","单价(元)","金额(元)","备注"]
[1,"DSP实验开发系统","国内有名的DSP实验箱研制厂商和TI芯片供货单位",null,"DSP多媒体开发系统硬件平台：\n1、DSP芯片：TMS320DM6446（DaVinci：ARM9+DM64X双核）；\n2、基本硬件资源：（最低配置要求）\n■ LCD显示屏（4.3\" LCD）；\n■ XDS560PLUS硬件仿真器；\n■ 外部存储：DDR2（32M×32位）；NAND Flash：64M×8位；\n■ Flash/多媒体卡接口（MMC/SD 卡接口）；\n■ UART接口（RS232与RS485）；\n■ Video接口（PAL/NTSC标准模拟视频输入口，PAL/NTSC标准模拟视频输出，支持VGA输出）；\n■ Audio接口（立体声输入／输出）；\n■ 数字IO（I/O：4入2出）；\n■ 以太网接口（10M/100M标准以太网）；\n■ USB接口（直接挂接U盘或无线设备，支持主从模式）；\n■ 总线扩展口（扩展EMIFA与VPEE总线）；\n■ 存储设备（40G 2.5英寸SATA硬盘）；\n■ JTAG接口（#14芯标准JTAG接口）；\nDSP多媒体开发软件资源：\n■ 开发套件（DaVinci Linux Develop Software）；\n■ DSP多媒体实验指导书；\n■ 多媒体数字实验源代码（H.264、MPEG4、JPEG、G.711、G.729、ACC、MP3等）；\n■ 教学资源光盘；","套",24,null,null,"投标公司需现场展示所投标类型的产品"]
["合计"]