{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["公寓楼网络工程设备招标采购清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"公寓楼网络工程设备招标采购清单","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"merged":[[0,0,0,9],[21,0,21,9]],"flags":["formulas_cached_only"]}
["安康学院学生公寓楼网络工程设备招标采购清单"]
["序号","设备名称","品  牌","型号","规格及主要技术指标","单位","数量","单价（元）","总价（元）","备注"]
[1,"交换机","思科/华三/锐捷",null,"交换容量≥192Gbps；IPv4/IPv6转发性能≥66Mpps；千兆电口数≥24；千兆SFP光口数≥4，可复用；支持可扩展万兆端口数≥2；支持IEEE 802.1Q VLAN、端口镜像、链路聚合，单向链路检测；支持静态路由、RIP V1/V2、OSPF、OSPFV3等路由协议；支持DHCPv6、ACLv6；支持BFD协议实现路由快速收敛；设备管理方面支持Telnet、Console、Web、RMON、SSHv2、SNMPv1/v2/v3；产品资质方面要求提供电信进网许可证(IPV4、IPV6)。","台",2,null,null,"汇聚交换机"]
[2,"交换机(48口)","思科/华三/锐捷",null,"IPv4/IPv6转发性能≥13.2Mpps；百兆电端口数≥48；千兆端口数≥2，光电复用，整机可扩展至4口千兆光电复用接口；支持端口汇聚，支持自动/手工汇聚；支持IPv6 Host；支持IPv6 ACL；支持DHCP Client、DHCP Snooping、DHCP Snooping Trust；支持基于MAC/IP的负载均衡；组播特性方面支持IGMP v1/v2/v3 Snooping；管理特性方面支持SNMPv1/v2/v3，提供MIB接口，支持WEB网管，支持TELNET、SSH登陆；支持Radius管理用户，支持电缆检测，支持端口环回检测；安全特性方面支持802.1x认证、支持防ARP欺骗、支持ARP报文按速率限速、支持MAC过滤、限制端口学习MAC地址数量；产品资质要求提供电信进网许可证。","台",12,null,null,"楼宇交换机；为维护与管理的便利性，必需为同一系列交换机产品"]
[3,"交换机（24口）","思科/华三/锐捷",null,"IPv4/IPv6转发性能≥6.5Mpps；百兆电端口数≥24；千兆端口数≥2，光电复用；整机可扩展至4口千兆光电复用接口；支持端口汇聚，支持自动/手工汇聚；支持IPv6 Host；支持IPv6 ACL；支持DHCP Client；DHCP Snooping；DHCP Snooping Trust；支持基于MAC/IP的负载均衡；组播特性方面支持IGMP v1/v2/v3 Snooping；管理特性方面支持SNMPv1/v2/v3，提供MIB接口，支持WEB网管，支持TELNET、SSH登陆，支持Radius管理用户，支持电缆检测，支持端口环回检测；安全特性方面支持802.1x认证，支持防ARP欺骗，支持ARP报文按速率限速，支持MAC过滤，限制端口学习MAC地址数量；产品资质方面要求提供电信进网许可证。","台",30,null,null,"楼宇交换机；为维护与管理的便利性，必需为同一系列交换机产品"]
[4,"\n交换模块\nMini-GBIC-LX\n","思科/华三/锐捷",null,"1000BASE-LX mini GBIC转换模块","个",2]
[5,"机柜","万通",null,"12U","个",6]
[6,"配线架","永鑫",null,"TE-PCM-2012R4548 / 24口超五类非屏蔽配线架","个",42]
[7,"双绞线跳线","永鑫",null,"TE-PC-UTPe-02org  Cat 5e非屏蔽跳线/橙色/1M/B类","根",1010]
[8,"水晶头","永鑫",null,"TE-PLUG-UT3P-R45/100只装","盒",11]
[9,"模块","永鑫",null,"TE-KCM-2013B-R45 Cat5e 超五类模块","个",960]
[10,"面板","永鑫",null,"TE-DBJ-07MIFP1WH欧式单孔面板(防尘式) (86*86mm)","个",960]
[11,"网线","永鑫",null,"TE-PC-UTPe-02org  Cat 5e非屏蔽双绞线","箱",11]
[12,"网线","永鑫",null,"TE-UTP-CAT 600 4BL 六类四对非屏蔽双绞线(305M)","箱",2]
[13,"室外光缆","立孚",null,"室外单模光缆（长度及纤芯数量据现场需要确定）","米",300]
[14,"光纤跳线","立孚",null,"SC-LC单模   ","根",5]
[15,"光纤跳线","立孚",null,"SC-LC多模   ","根",5]
[16,"光缆熔接","立孚",null,null,"芯",4]
[17,"网络机柜","图腾/IBM/DELL",null,"42U标准机柜（含防雷的PDU电源、侧面板、黑色)","个",3]
[18,"服务器机柜","图腾/IBM/DELL",null,"42U标准机柜（含防雷的PDU电源、侧面板、黑色)","个",2]
[19,"合计"]
["说明：1、每套方案中，交换设备请在提供的备选品牌中选择一个品牌；\n             2、本次工程不含楼宇综合布线工程。\n             3、完工后必须提供布线示意图及设备、配线架编号、交换机端口对应表等技术文档。\n             4、所有设备上架，应免费按甲方要求调试接通并测试通过。"]