{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["基础化学实验室","综合实验室 (2)"],"not_rendered":{"external_links":1,"defined_names":9},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"基础化学实验室","index":0,"n_rows":30,"n_cols":11,"rows_kept":30,"merged":[[0,0,0,10],[1,0,1,10],[28,0,28,1],[29,0,29,10]],"flags":["formulas_cached_only"]}
["安康学院化学化工系实验室仪器设备采购清单"]
["第一标段：基础化学实验室仪器设备"]
["序号","仪器名称","品牌","参考型号","规格","生产厂家","单位","数量","单价(元）","金额(元）","备注"]
[1,"电子天平",null,"BL310","310g(0.01g)",null,"台",4,null,null,"进口"]
[2,"电子天平",null,"BS210S\n或AL204","0.0001g,自动显示数据",null,"台",4,null,null,"进口"]
[3,"电炉",null,"DK-98-1","2KW",null,"个",30]
[4,"电吹风",null,"HP4819\n或HP4887","1Kw",null,"个",5]
[5,"电导率仪",null,"DDS-11At\n或AZ-8303",null,null,"台",2]
[6,"可见分光光度计",null,"722E","325-1000nm；±2nm；重复性<1nm，光谱带宽5nm；吸光度范围-0.097—2.000A",null,"台",2]
[7,"磁力搅拌器",null,"JB-1B\n或 HZ79-1","数显，温度可调",null,"台",10]
[8,"真空保温杯",null,"304优质不锈钢","300-400ml",null,"个",10]
[9,"旋转蒸发仪",null,"RE-52-AA \n或RE52-AAA","转速0-150转/分；自动控温0-95度，手轮升降；电子调速",null,"台",2]
[10,"紫外检测仪",null,"WD-9403E\n或ZF-6","254, 365(nm)",null,"个",2]
[11,"离心机",null,"80-1","4000转每分20ml×6",null,"台",2]
[12,"离心机",null,"DL-8000B-C3或80","角式 10ml×12",null,"台",5]
[13,"超声波清洗仪",null,"HS-120D\n或KQ2200E","120W",null,"台",1]
[14,"显微熔点测定仪",null,"XT3A","10X或5X；50-300度；最小分度值1度；数显；程控；精度±1%",null,"台",1]
[15,"数显自动旋光仪",null,"WZZ-2A\n或WZZ-2B","测量范围±45度；数显最小值0.005度",null,"台",2]
[16,"水浴锅",null,"DK-2000-IIIL","数显智能型单列双孔",null,"个",11]
[17,"铂丝",null,"0.2mm",{"v":0.9999,"d":"99.99%"},null,null,"4g"]
[18,"计算器",null,"DRS-12","科学计数    ",null,"个",10]
[19,"器皿柜",null,null,"灰色；2×0.9×0.45m",null,"个",5,null,null,"杨凌天工或西安博思博生产"]
[20,"手持GPS",null,"Triton500","附中文说明书",null,"个",2]
[21,"等高线地貌模型",null,null,"500×300㎜；高分子材料附文字说明地貌特征",null,"个",1]
[22,"丹霞地貌模型",null,null,"500×300㎜；高分子材料附文字说明地貌特征",null,"个",1]
[23,"喀斯特地貌模型",null,null,"500×300㎜；高分子材料附文字说明地貌特征",null,"个",1]
[24,"海岸地貌模型",null,null,"500×300㎜；高分子材料附文字说明地貌特征",null,"个",1]
[25,"立体雕塑教学地球仪",null,"xy8001 中文450mm","高分子玻璃钢树脂",null,"个",1]
["合    计"]
["说明：单价3000元以上设备须提供生产厂家或总代理商的授权书。"]

{"sheet":"综合实验室 (2)","index":1,"n_rows":46,"n_cols":11,"rows_kept":46,"merged":[[0,0,0,10],[1,0,1,10],[44,0,44,1],[45,0,45,10]],"flags":["formulas_cached_only"]}
["安康学院化学化工系实验室仪器设备采购清单"]
["第二标段：综合实验室（2）仪器设备"]
["序号","仪器名称","品牌","参考型号","规格","厂家","单位","数量","单价(元）","金额(元）","备注"]
[1,"箱式电阻炉",null,"SX2-2.5-10","200X120X80,工作温度1000℃",null,"台",1]
[2,"电子天平",null,"BS210S或AL204","0.0001g,自动显示数据",null,"台",2]
[3,"连续变倍体视显微镜",null,"XYH03或XTL-H","放大倍数7X~45X",null,"台",2]
[4,"水热反应釜",null,"不锈钢，聚四氟乙烯内胆","50ml、30ml（各6个）",null,"个",12]
[5,"自动低压液相色谱分离层析仪",null,"2001-C-I(六件套)或2001-A-II（六件套）　","电脑和打印机（标准配置254nm、280nm同时检测）",null,"台",1]
[6,"研  钵",null,null,"φ90，玛瑙",null,"台",6]
[7,"数显旋光仪",null,"WZZ-2B或CN61M/WZZ-1S","微机数显，精度：≤0.005℃",null,"台",2]
[8,"水分测定仪",null,"SC69-02C或MA150 MA35（德国）","100g/0.1mg",null,"台",2]
[9,"显微熔点测定仪",null,"WRS-1B或XT6","微机，数显，最小读数单位：0.1℃",null,"台",1]
[10,"离心机",null,"TGL-18C-C或德国sigma3k15","最大容量4×200ml/4×250ml",null,"台",1]
[11,"超声波清洗仪",null,"HS-120D、KQ2200E","可控温，功率1200",null,"台",2]
[12,"玻璃色谱柱",null,"玻璃","直径10cm2个；\n直径5cm10个；\n直径2.5cm10个；\n直径1cm30个",null,"套",52]
[13,"索氏提取器",null,"SXT-02或SCT-02","含油量在0.5%-60%范围内的各种样品",null,"台",10]
[14,"中草药粉碎机",null,"FW177","一次投入量：400g，粉碎60-120目",null,"台",2]
[15,"小型电动离心机",null,80,"容量：6×5",null,"台",2]
[16,"小型电动离心机",null,80,"容量：6×2.5",null,"台",2]
[17,"电热恒温干燥箱（带鼓风）",null,"202-O-S\\WG71\nWHG-9023A或WH20","数显，温度范围10-200OC（±2.0%）",null,"台",2]
[18,"旋转蒸发仪",null,"R501B或RE-5205","5升，伸降水浴锅，转速数显",null,"台",1,null,null,"带配套胶管"]
[19,"旋转蒸发仪",null,"RE-52-AA 或RE52-A","小型常规配置，伸降水浴锅，转速数显",null,"台",2,null,null,"带配套胶管"]
[20,"台式冷冻干燥机",null,"FD—1或TF-18S","普通，≤-45℃，数字显示    冷阱温度及真空度，四层托盘冻干面积0.1m2",null,"台",1]
[21,"智能崩解仪",null,"ZB-1C","两杯式",null,"台",2]
[22,"实验台",null,null,"钢架结构，台面板为黑色理化板，0.75×2×0.8m",null,"个",14,null,null,"杨凌天工或西安博思博生产"]
[23,"小型多功能制丸机",null,"ZW-200或DZ-20C","5-30mm（学生实验用）",null,"台",2]
[24,"小型v形混合机",null,"小型v形","（学生实验用）",null,"台",2]
[25,"紫外可见分光光度计",null,"SP-19017200或TU-1901/TU-1900　","含电脑（数据处理平台、打印机）",null,"台",1]
[26,"小型压片机",null,"TDP-1.5T","580×450×625毫米3600片/时\n（学生实验用）",null,"台",2]
[27,"手工胶囊填充板、定量数片板",null,"1#，2#，3#，400孔，各2个","1000粒/时（学生实验用）",null,"个",6]
[28,"小型制粒机",null,"YK-60，不锈钢","（学生实验用）",null,"台",2]
[29,"电吹风",null,"HP4819或HP4887 ",null,null,"个",5]
[30,"调温万用电炉",null,"DK-98-1","800-1000W",null,"台",10]
[31,"层析缸",null,null,"15×5×15cm，玻璃",null,"个",6]
[32,"紫外分析仪",null,"WD-9403E","254, 365nm",null,"个",2]
[33,"中草药粉粹机",null,"FY130或FW-177","1500W，60-200目",null,"台",2]
[34,"循环水真空泵",null,"SHE-Ⅲ","不锈钢，台式",null,"台",2]
[35,"水浴锅",null,"DK-2000-IIIL或DRS-12","数显智能型单列双孔",null,"个",3]
[36,"电热套",null,"PTHW","控温精度：±5℃",null,"台",6]
[37,"磁力搅拌器",null,"JB-1B/ HZ79-1","500 /1000 ML",null,"台",8]
[38,"电动喷雾器/喷雾显色箱",null,"YOKO-PN/YOKO-PX或 YK-DN/YK-PX","PN Ⅱ 型：功率 80W \n排气量 90L /mm ",null,"台",1]
[39,"投影仪",null,"松下、ESPON、SONY","投影方式：正投/背投 LCD投影 不小于3000流明，标准分辨率1024*768  对比度 400：1 屏幕比例 16：9 、4：3  灯泡寿命不小于2500小时，可直接断电，支持工作状态读取，具有强光感应功能。",null,"台",1,null,null,"便携式"]
[40,"幕布",null,"红叶","80寸，白塑或玻珠，移动式带支架",null,"套",1]
[41,"笔记本电脑",null,"戴尔/联想/HP商用机","英特尔® 酷睿™ 2双核处理器 P8600/2GB/250GB/内置DVD刻录机/12.1LCD/三年保修（黑色/带笔记本专用包/鼠标）带正版WINDOWS操作系统",null,"台",1]
["合计"]
["说明：单价3000元以上设备须提供生产厂家或总代理商的授权书。"]